V5.07.02b1

New functionality
RGB() function now accepts GREY

New Option can help to setup running without a battery.
OPTION RESTART [0|1|2]

Option.Restart is save in the Options.
It can have three values.
0 - This is the default value set by MMBasic at power up or OPTION RESET.
1 - This is set only whenever the OPTION SAVE command finds it at 0
2 - This can only ever be set explicitly by a MMBasic program with command
   OPTION RESTART 2
The value of Option.Reset can be read  by MM.INFO(RESTART)

Bug Fixes
Fixes Out of Memory error when EDIT is invoke with OPTION LCDPANEL CONSOLE set. (Non SSD1963 panels)
Fixes double spacing corruptiing the Fullscreen Editor with OPTION LCDPANEL CONSOLE set.


V5.07.02b0
MMBasic MUST be reset after loading this firmware. i.e. Hold K1 while applying power.

New functionality
Many changes- See initial Armmite F4 5.07.02 betas TBS thread for a summary. Also the Armmite F4 User Manual Change Log section.

Bug Fixes
See initial Armmite F4 5.07.02 betas TBS thread for a summary.

